

|  |
| --- |
|  |

ONIE Certification Test Procedure

Contents

[List of Changes 3](#_Toc391320281)

[License 4](#_Toc391320282)

[Background 5](#_Toc391320283)

[Introduction 5](#_Toc391320284)

[ONIE Specification 5](#_Toc391320285)

[Prerequisites 5](#_Toc391320286)

[Board EEPROM Information Format 5](#_Toc391320287)

[Hardware Face Plate and FRU Numbering 8](#_Toc391320288)

[Hardware Documentation 9](#_Toc391320289)

[Access to ONIE images 9](#_Toc391320290)

[Asset Tracking and Labeling 9](#_Toc391320291)

[NOS image discovery and Installation 10](#_Toc391320292)

[Default File Name Search Order 10](#_Toc391320293)

[Statically configured (passed from boot loader) 10](#_Toc391320294)

[Local file systems (USB for example) 11](#_Toc391320295)

[Exact URLs from DHCPv4 11](#_Toc391320296)

[Inexact URLs based on DHCP responses 11](#_Toc391320297)

[DHCP Reference Information 12](#_Toc391320298)

[HTTP Requests and Headers 13](#_Toc391320299)

[IPv6 neighbors 14](#_Toc391320300)

[TFTP waterfall 14](#_Toc391320301)

[NOS Uninstallation 15](#_Toc391320302)

[Update ONIE 15](#_Toc391320303)

[Default File Name Search Order 15](#_Toc391320304)

[Statically configured (passed from boot loader) 16](#_Toc391320305)

[Local file systems (USB for example) 16](#_Toc391320306)

[Exact URLs from DHCPv4 16](#_Toc391320307)

[Inexact URLs based on DHCP responses 16](#_Toc391320308)

[IPv6 neighbors 16](#_Toc391320309)

[TFTP waterfall 16](#_Toc391320310)

[Rescue Mode 17](#_Toc391320311)

[Execution Environment 17](#_Toc391320312)

[ONIE Testing 18](#_Toc391320313)

[Test Environment 18](#_Toc391320314)

[Dead on Arrival Testing 19](#_Toc391320315)

[Manual Testing 19](#_Toc391320316)

[Preliminary 19](#_Toc391320317)

[NOS image discovery and Installation 21](#_Toc391320318)

[NOS Uninstallation 22](#_Toc391320319)

[Update ONIE 22](#_Toc391320320)

[Rescue Mode 23](#_Toc391320321)

[Appendix A – dhcpd.conf example file 25](#_Toc391320322)

[Table 1- Layout of entire EEPROM block 6](#_Toc391320323)

[Table 2 - Type Code Value Definitions 8](#_Toc391320324)

[Table 3 - DHCP Options for Exact URL 11](#_Toc391320325)

[Table 4 - DHCP Options used for Inexact URLs 12](#_Toc391320326)

[Table 5 - DHCP Request Options 12](#_Toc391320327)

[Table 6 - VIVSO Namespace Option Codes 13](#_Toc391320328)

[Table 7 - DHCP Parameter Request List Options 13](#_Toc391320329)

[Table 8 - HTTP Headers 14](#_Toc391320330)

[Table 9 - Installer Core Environment Variables 17](#_Toc391320331)

[Table 10 - Installer DHCP Environment Variables 18](#_Toc391320332)

[Table 11- ONIE Variables from Device 21](#_Toc391320333)

# List of Changes

|  |  |  |  |
| --- | --- | --- | --- |
| Version | Changes | Name | Date |
| 0.1 | Initial Draft | Carlos Cardenas | 2014/05/27 |
| 0.2 | Review, feedback, add hardware test | Thao Nguyen | 2014/06/05 |
| 0.3 | Added:   * Testing Environment * Manual Testing | Carlos Cardenas | 2014/06/10 |
| 0.4 | Incorporate RFC 2119 language, clarify port enumeration, labeling requirements | Matt Peterson | 2014/06/11 |
| 0.5 | Added:   * Test Number references * Example dhcpd.conf file | Carlos Cardenas | 2014/06/25 |
| 0.6 | Added:   * Clarified USB install to be optional (based on HW availability) * Clarified that “luggage tag” on device is to include additional space for end user’s asset tracking system | Carlos Cardenas | 2014/07/24 |
| 0.7 | Corrected:   * Static Install * Static Update   To use onie\_debugargs | Carlos Cardenas | 2014/08/22 |
| 0.8 | Corrected:   * DHCP option for Server IP * CPU architecture name for x86\_64 | Carlos Cardenas | 2015/02/03 |

# License

As of September 12, 2013, the following persons or entities (according to alphabet sequence) have made this Specification available under the Open Web Foundation Final Specification Agreement (OWFa 1.0), which is available at http://www.openwebfoundation.org/legal/the-owf-1-0-agreements/owf-contributor-license-agreement-1-0---copyright-and-patent.

University of Texas at San Antonio

Cumulus Networks

Facebook, Inc.

You can review the signed copies of the Open Web Foundation Agreement Version 1.0 for this Specification at http://opencompute.org/licensing/, which may also include additional parties beyond those listed above.

Your use of this Specification may be subject to other third party rights. THIS SPECIFICATION IS PROVIDED "AS IS." The contributors expressly disclaim any warranties (express, implied, or otherwise), including implied warranties of merchantability, non-infringement, fitness for a particular purpose, or title, related to the Specification. The entire risk as to implementing or otherwise using the Specification is assumed by the Specification implementer and user. IN NO EVENT WILL ANY PARTY BE LIABLE TO ANY OTHER PARTY FOR LOST PROFITS OR ANY FORM OF INDIRECT, SPECIAL, INCIDENTAL, OR CONSEQUENTIAL DAMAGES OF ANY CHARACTER FROM ANY CAUSES OF ACTION OF ANY KIND WITH RESPECT TO THIS SPECIFICATION OR ITS GOVERNING AGREEMENT, WHETHER BASED ON BREACH OF CONTRACT, TORT (INCLUDING NEGLIGENCE), OR OTHERWISE, AND WHETHER OR NOT THE OTHER PARTY HAS BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

# Background

## Introduction

ONIE or the Open Network Install Environment is second stage boot loader to facilitate the installation of operating systems. The original implementation was built to install network operating systems on “bare metal” or whitelabel network switches. The architecture is geared to preserve a preliminary “BIOS” or initial system ROM to bring up the system (such as UBoot for PPC or SeaBIOS for x86); while ONIE functions exclusively to discover network, fetch an OS image, and execute an unattended installer. This document serves as foundation for vendors or suppliers who wish to certify their ONIE implementation under the support of the Open Compute Project.

The defined specification follows [RFC 2119](http://tools.ietf.org/html/rfc2119) language for the terms “MUST”, “MUST NOT”, “SHOULD”, “SHOULD NOT”, and “MAY”.

# ONIE Specification

## Prerequisites

The ONIE firmware has modest hardware requirements that are required before ONIE can be used as intended in this specification.

### Board EEPROM Information Format

Each ONIE system MUST include an EEPROM which contains various system parameters assigned by the manufacturer. This EEPROM includes information such as the MAC address(es) allocated to the system, the serial number, the date of manufacturer, manufacturer name etc. The name of the EEPROM format specified here is TlvInfo, because the information contained in the EEPROM is found in TLVs, or **T**ype **L**ength and **V**alue fields.

#### Definition of the TlvInfo EEPROM Format

The first eight bytes in the EEPROM MUST be a NULL-terminated ASCII string TlvInfo. This identification string can be used as a simple, preliminary check that the EEPROM conforms to the TlvInfo format defined here. Additional validation checks should be performed to validate that the TlvInfo format is really being used, such as validating the CRC. But this string provides a good clue, when debugging or dumping memory, that what follows is in the TlvInfo EEPROM format.

The identification string MUST BE followed by a single-byte version value. This value is set to 0x01 for the TlvInfo EEPROM format described in this document. Since the format described herein is very flexible and extensible, this value is not expected to ever change, but is included just in case. Software SHOULD NOT assume anything about the format of the data that follows this byte if it has not been written to support the version it reads from this value. The values 0x00 and 0xFF are reserved and will never be used.

The version field MUST BE followed by two bytes, which give the total length of the data that follows. This field is in big endian order and includes the cumulative length of all of the TLV fields that follow. This field MAY be used to determine the amount of data to read, if the EEPROM data is read in bulk, following the first 11 bytes. This field can also be used to determine the location of the CRC, since the CRC-32 TLV is fixed length and always the last TLV in the EERPOM.

The total length field MUST BE followed by the EEPROM system data, known as *TLV fields*. Each TLV field is composed of three sub-fields: a type code field, a length field, and a value field, in that order.

* **Type** code: This is a single byte that defines the type and format of the value field. These types are defined in the table below. Since these type codes can be added over time, software that does not understand a particular type code MUST treat the value field as opaque data, not assigning any meaning to its type or format. Type codes 0x00 and 0xFF are reserved and will never be used. This allows for up to 254 type codes.
* **Length**: This is a single byte that contains the number of bytes in the value field. Valid values of this field range from 0 to 255. A length of zero means that there is no value field associated with this type code. In that case, the byte following the length field is the first byte of the next TLV, its type code field.
* **Value**: This field contains the value for the specified type code. It may range in size from 0 to 255 bytes. The format of this field is defined, below, for each of the individual type codes. Because each TLV contains a length field, ASCII strings are not NULL-terminated, unless otherwise specified as described below.

Only the CRC-32 TLV is required to be present by this specification, but some systems may not initialize properly without the presence of other fields. The CRC-32 TLV must occur last. This field can be quickly found at the following offset in the EEPROM by adding 11 (the length of the fixed header information) + the value of the total length field - 6 (the length of the CRC-32 TLV field).

The total length of the TlvInfo EEPROM data, from the first byte of the identification string to the last byte of the CRC TLV, must be less than or equal to 2048 bytes.

The layout of the entire EEPROM block looks like:

|  |  |  |
| --- | --- | --- |
| Field Name | Size in Bytes | Value |
| ID String | 8 | “TlvInfo” |
| Header Version | 1 | 0x01 |
| Total Length | 2 | Total number of bytes that follow |
| TLV 1 | Varies | The data for TLV 1 |
| TLV 2 | Varies | The data for TLV 2 |
| ..... | ..... | ..... |
| TLV N | Varies | The data for TLV N |
| CRC-32 TLV | 6 | Type = 0xFE, Length = 4, Value = 4 byte CRC-32 |

Table - Layout of entire EEPROM block

#### Type Code Values

The following type codes are defined.

|  |  |  |  |
| --- | --- | --- | --- |
| Type Code | Length | Description | Format |
| 0x00 | None | Reserved | This type code is illegal and will never be used, so that it will be easy to detect if a portion of the EEPROM is erased. |
| 0x21 | Variable | Product Name | An ASCII string containing the product name. |
| 0x22 | Variable | Part Number | An ASCII string containing the vendor’s part number for the device. |
| 0x23 | Variable | Serial Number | An ASCII string containing the serial number of the device. |
| 0x24 | 6 bytes | MAC #1 Base | Six bytes containing the base MAC address for this device. The first three bytes contain the OUI of the assigning authority. |
| 0x25 | 19 bytes | Manufacture Date | An ASCII string that specifies when the device was manufactured. The format of this string is: MM/DD/YYYY HH:NN:SS where MM is the month (01-12), DD is the day of the month (01-31), YYYY is the year, HH is the hour (00-23), NN is the minute (00-59), and SS is the second (00-59). |
| 0x26 | 1 byte | Device Version | A single byte indicating the version, or revision, of the device. |
| 0x27 | Variable | Label Revision | An ASCII string containing the label revision. |
| 0x28 | Variable | Platform Name | An ASCII string which identifies a CPU subsystem (CPU, architecture, DRAM, NOR flash). Very useful when the CPU resides on a daughter card. Typically this includes <arch>-<machine>-<machine\_revision>. |
| 0x29 | Variable | ONIE Version | An ASCII string containing the version of the ONIE software installed by the manufacturer. |
| 0x2A | 2 bytes | Num MACs | A two-byte big-endian unsigned integer describing the number of sequential MAC addresses allocated to this device, starting with the value specified in the MAC #1 Base TLV (code 0x2A). Valid values for this field range from 1 to 65535. |
| 0x2B | Variable | Manufacturer | An ASCII string containing the name of the entity that manufactured the device. |
| 0x2C | 2 bytes | Country Code | A two-byte ASCII string containing the ISO 3166-1 [alpha-2 code](http://www.iso.org/iso/country_codes/iso_3166_code_lists/country_names_and_code_elements.htm) of the country where the device was manufactured. |
| 0x2D | Variable | Vendor | The name of the vendor who contracted with the manufacturer for the production of this device. This is typically the company name on the outside of the device. |
| 0x2E | Variable | Diag Version | An ASCII string containing the version of the diagnostic software. |
| 0x2F | Variable | Service Tag | An ASCII string containing a vendor defined service tag. |
| 0xFD | Variable | Vendor Extension | This type code allows vendors to include extra information that is specific to the vendor and cannot be specified using the other type codes. The format of this value field is a four byte IANA enterprise number, followed by a vendor defined string of bytes. The format of the string of bytes is entirely up to the vendor, except that it can be, at most, 255 bytes long, including the [IANA enterprise number](http://www.iana.org/assignments/enterprise-numbers/enterprise-numbers). If more space is needed, then multiple TLVs with this type code can be used. |
| 0xFE | 4 bytes | CRC-32 | A four-byte CRC which covers the EEPROM contents from the first byte of the EEPROM (the “T” in the “TlvInfo” identification string) to the length field of this TLV, inclusive. This CRC uses the crc32 algorithm (see Python’s binascii.crc32() function). |
| 0xFF | None | Reserved | This type code is illegal and will never be used, so that it will be easy to detect if a portion of the EEPROM is erased. |

Table - Type Code Value Definitions

#### Note about MAC Addresses

A very critical characteristic of a switching platform EEPROM is the number of MAC addresses allocated to the machine. The firmware requires allocating 1 MAC address for every *serdes* on the box.

For example, consider a machine that has one Ethernet management port and a switching ASIC with 48x10G ports plus 6x40G ports. Each 40G port could be broken out into 4x10G ports. Therefore, the total number of MAC addresses this machines requires is:

1 -- Ethernet management port

48 -- 1 for each 48x10G port

24 -- 4 for each 6x40G port

-----------------------------

73 Total MACs

To encode that in the EEPROM, set TLV code 0x2A (Num MACs) to 73.

### Hardware Face Plate and FRU Numbering

The following conventions for face plate and FRU numbering shall be used on the sheet metal silkscreen for the switch:

1. All enumerations start at 1, not 0. This is due to the historical nature of ONIE, where the first supported platforms where ODM based networking hardware, which chose this scheme.
2. Switch ports are labeled starting with the number “1”. This scheme assumes facing at the front of the switch, or whichever side has the most predominate number of ports.
3. Switch ports are labeled top to bottom, left to right. For example, consider a 48 port switch with two rows of switch ports (two rows of 24 ports). The ports along the top row are labeled “1, 3, 5…47” and the bottom row is labeled “2, 4, 8..48”. Port should be labeled only with a number designation, no “eth#” or “swp#” pre or appended name – as each operating system my name this differently.
4. Field Replaceable Units (FRUs) are labeled starting with the number “1”. This typically applies to field pluggable power supplies, fan modules, or other expansion slots. For example, a system with 2 PSUs and 3 fan modules would label the PSUs “1, 2” and the fans “1, 2, 3”.

### Hardware Documentation

As ONIE becomes ubiquitous in switching hardware, the hardware vendor shall include a one page (two sides printed) **Quick Start Guide** flyer.

This flyer MUST include at least the following:

* Installed ONIE version number and certification number/date
* Stencil of front and rear switch view that calls out or arrows for the follow locations:
  + First usable management Ethernet port
  + Out of band serial or console port
  + FRU’s (such as fans and power supplies, enumerated as specified above)
* If the baud rate or settings information is changed from the default (115200 baud, 8/n/1 – no flow control), this data should be noted.
* Console port pin out or wiring scheme to a standard DB9 cable.
* Generic ONIE installation instructions (visual of network waterfall, file name discovery) – pointers to the ONIE website or similar tiny URL with more verbose instructions. A template of this graphical element will be available in a future specification standard.
* Generic ONIE debugging (ssh/telnet access, syslog) – pointers to ONIE website.

### Access to ONIE images

Over the course of the lifetime of a given switch product, new features may be released in upstream ONIE that a vendor may want to make available to all of their relevant products.

* All ONIE released and upgrade images much be made available from a public accessible HTTP and/or FTP server. Such access MUST be freely accessible without any credentials or special login information.
* All shipping, archival, and upgrades versions SHOULD be available to download.
* Such files should be offered in a directory tree starting with the SKU name, followed by ONIE version number.

### Asset Tracking and Labeling

Asset tracking is a vital part of an operator’s work flow and as such, the following asset tracking labels are required:

* Human and machine readable barcodes that represent the first usable Ethernet management port (usually eth0) MAC address, system serial number, product family or SKU identification and CPU ID. Acceptable barcode encoding MUST be: Code 38, Code 128, or QR Code as ASCII text. Such encoding between human and machine-readable should be consistent (for example, a serial number printed as ASCII but encoded as HEX is not acceptable).
* For products that will be offered in a 2 or 4 post rack environment, these labels SHOULD be available on the sides of the switches, **not** on the top or bottom of the switch – as to make them readable once racked. A perfect example would be the “luggage tag” that many server vendors currently use.
* Wherever the asset locators are placed on the device there needs to be enough space for an end user to place their own asset locators. An ideal area is a “luggage tag” with enough space for an end user’s asset locator.
* On platforms that support the SMBIOS/DMI standard, the serial number and product family / SKU identifier information must be encoded to match human-readable labels. For example, the encoding of the serial number (SMBIOS type 1, offset 07h) field MUST NOT be null or fake (123456789).

## NOS image discovery and Installation

The firmware is required to discover a NOS image through the following methods (in order):

1. Statically configured (passed from boot loader)
2. Local file systems (USB for example)
3. Exact URLs from DHCPv4
4. Inexact URLs based on DHCP responses
5. IPv6 neighbors
6. TFTP waterfall

Once the image has been downloaded, the firmware is required to perform the installation of the NOS. At the end of installation, the firmware shall not attempt to auto discover another image, unless instructed to by the NOS or user but rather should boot the NOS installed.

In the event of an installation failure, the firmware shall repeat the NOS image discovery and installation process.

### Default File Name Search Order

In a number of the following methods, ONIE searches for default file names in a specific order. All the methods use the same default file names and search order, which are described in this section.

The default installer file names are searched for in the following order:

1. onie-installer-<arch>-<vendor>\_<machine>-r<machine\_revision>
2. onie-installer-<arch>-<vendor>\_<machine>
3. onie-installer-<vendor>\_<machine>
4. onie-installer-<arch>
5. onie-installer

### Statically configured (passed from boot loader)

The firmware shall provide this static method as an engineering function to be used during the porting of ONIE to a new platform. To use this method, a statically configured installer URL (install\_url) shall be set by the user on the kernel command line argument prior to booting ONIE. Additional kernel command line arguments can be added by setting the onie\_debugargs environment variable.

### Local file systems (USB for example)

The firmware shall provide a method to identify a locally attached storage device to obtain a NOS installer. This method is intended for the case where the NOS installer is available on a USB memory stick (if supported by the device) plugged into the front panel. The supported file systems the firmware will support shall be vfat (common on commercially available USB sticks) and ext2.

The general algorithm for locating the installer on local storage proceeds as follows:

foreach $partition in /proc/partitions {

if able to mount $partition then {

if default file name exists {

Add partition to found\_list

}

}

}

foreach $partition in found\_list {

Run installer from $partition

}

### Exact URLs from DHCPv4

The DHCP options discussed below, provide a number of ways to express the exact URL of the NOS installer. When interpreting URLs, the firmware accepts the following URI schemes:

* http://server/path/...
* https://server/path/...
* ftp://server/path/...
* tftp://server/path/…

The following options can be used to form the exact URL.

|  |  |  |
| --- | --- | --- |
| Option | Name | Comments |
| 125 | VIVSO | The installer URL option (code = 1). Options yields an exact URL. |
| 114 | Default URL | Intended for HTTP, but other URLs are accepted. |
| 150 + 67 | TFTP server IP and TFTP bootfile | Both options are required for an exact URL. |
| 66 + 67 | TFTP server name and TFTP bootfile | Both options are required for an exact URL. Requires DNS. |

Table - DHCP Options for Exact URL

### Inexact URLs based on DHCP responses

The firmware can find an installer using partial DHCP information by using a default sequence of URL paths and default file names in conjunction with partial DHCP information available to find an installer.

The following DHCP option responses are used to locate an installer in conjunction with the default file names:

|  |  |  |
| --- | --- | --- |
| DHCP Options | Name | URL |
| 67 | TFTP Bootfile | Contents of bootfile |
| 72 | HTTP Server IP | http://$http\_server\_ip/${onie\_default\_installer\_names} |
| 66 | TFTP Server IP | http://$tftp\_server\_ip/${onie\_default\_installer\_names} |
| 54 | DHCP Server IP | http://$dhcp\_server\_ip/${onie\_default\_installer\_names} |

Table - DHCP Options used for Inexact URLs

### DHCP Reference Information

DHCP provides a powerful and flexible mechanism for specifying the installer URL. During the DHCP request, the firmware sets a number of options to help the DHCP server determine an appropriate response. The following table illustrates what options are set during the request phase.

|  |  |  |  |
| --- | --- | --- | --- |
| Option | Name | ISC option-name | RFC |
| 60 | Vendor Class Identifier | vendor-class-identifier | [RFC 2132](http://tools.ietf.org/html/rfc2132) |
| 77 | User Class | user-class | [RFC 2132](http://tools.ietf.org/html/rfc2132) |
| 125 | Vendor-Identifying Vendor-Specific Information | vivso | [RFC 3925](http://tools.ietf.org/html/rfc3925) |
| 55 | Parameter Request List | dhcp-parameter-request-list | [RFC 2132](http://tools.ietf.org/html/rfc2132) |

Table - DHCP Request Options

#### Vendor Class Identifier – Option 60

The vendor class identifier option is the concatenation of two strings, separated by the colon ‘:’ character.

1. The static string onie\_vendor
2. <arch>-<vendor>\_<machine>-r<machine\_revision>

For example, using the example PowerPC machine, the string would be:

onie\_vendor:powerpc-VENDOR\_MACHINE-r0

At this time, the only valid values for CPU architecture are:

* powerpc
* x86\_64

#### User Class – Option 77

The user class option is set to the static string

onie\_dhpc\_user\_class

#### Vendor-Identifying Vendor-Specific Information – Option 125

The VIVSO option allows for custom namespaces, where the namespace is identified by the 32-bit IANA Private Enterprise Number. The firmware currently uses the enterprise number 42623 to identify its custom namespace.

The option codes within the firmware namespace have a size of 1 byte. The option payload length is also 1 byte.

Within this namespace, the following option codes are defined:

|  |  |  |  |
| --- | --- | --- | --- |
| Option Code | Name | Type | Example |
| 1 | Installer URL | string | http://10.0.0.1/nos\_installer.bin |
| 2 | Updater URL | string | http://10.0.0.1/onie\_update.bin |
| 3 | Platform Name | string | VENDOR\_MACHINE |
| 4 | CPU Architecture | string | powerpc |
| 5 | Machine Revision | string | 0 |

Table - VIVSO Namespace Option Codes

#### Parameter Request List – Option 55

The parameter request list option encodes a list of requested options. The firmware requests the following options:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Option | Name | ISC option-name | Option Type | RFC | Example |
| 1 | Subnet Mask | subnet-mask | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 255.255.255.0 |
| 3 | Default Gateway | routers | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 10.0.0.1 |
| 6 | Domain Server | Domain-name-servers | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 10.0.0.1 |
| 7 | Log Server | log-servers | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 10.0.0.1 |
| 12 | Hostname | host-name | string | [2132](http://tools.ietf.org/html/rfc2132) | switch-01 |
| 15 | Domain Name | domain-name | string | [2132](http://tools.ietf.org/html/rfc2132) | example.com |
| 42 | NTP Servers | ntp-servers | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 10.0.0.1 |
| 54 | DHCP Server Identifier | dhcp-server-identifier | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 10.0.0.1 |
| 66 | TFTP Server Name | tftp-server-name | string | [2132](http://tools.ietf.org/html/rfc2132) | bootserver |
| 67 | TFTP Bootfile Name | bootfile-name or filename | string | [2132](http://tools.ietf.org/html/rfc2132) | tftp/installer.sh |
| 72 | HTTP Server IP | www-server | dotted quad | [2132](http://tools.ietf.org/html/rfc2132) | 10.0.0.1 |
| 114 | Default URL | default-url | string |  | http://server/install |
| 150 | TFTP Server IP Address | next-server | dotted quad |  | 10.0.0.2 |

Table - DHCP Parameter Request List Options

### HTTP Requests and Headers

All HTTP requests made by the firmware include a set of standard HTTP headers, which an HTTP automation system could utilize. The headers sent on each HTTP request are:

|  |  |  |
| --- | --- | --- |
| Header | Value | Example |
| ONIE-SERIAL-NUMBER | Serial number | XYZ123004 |
| ONIE-ETH-ADDR | Management MAC address | 08:9e:01:62:d1:93 |
| ONIE-VENDOR-ID | 32-bit IANA Private Enterprise Number | 12345 |
| ONIE-MACHINE | <vendor>\_<machine> | VENDOR\_MACHINE |
| ONIE-MACHINE-REV | <machine\_revision> | 0 |
| ONIE-ARCH | CPU architecture | powerpc |
| ONIE-OPERATION | ONIE mode of operation | os-install or onie-update |
| ONIE-VERSION | Version of ONIE | onie/1.0 (2.6.13) |

Table - HTTP Headers

### IPv6 neighbors

The firmware shall also query its IPv6 link-local neighbors via HTTP for an installer. The general algorithm follows:

Ping6 the “all nodes” link local IPv6 multicast address, ff02::1

For each responding neighbor, try to download the default file names from the root of the web server

The following is an example of URLs used by this method:

http://fe80::4638:39ff:fe00:139e%eth0/onie-installer-powerpc-VENDOR\_MACHINE-r0

http://fe80::4638:39ff:fe00:139e%eth0/onie-installer-powerpc-VENDOR\_MACHINE

http://fe80::4638:39ff:fe00:139e%eth0/onie-installer-VENDOR\_MACHINE

http://fe80::4638:39ff:fe00:139e%eth0/onie-installer-powerpc

http://fe80::4638:39ff:fe00:139e%eth0/onie-installer

http://fe80::4638:39ff:fe00:2659%eth0/onie-installer-powerpc-VENDOR\_MACHINE-r0

http://fe80::4638:39ff:fe00:2659%eth0/onie-installer-powerpc-VENDOR\_MACHINE

http://fe80::4638:39ff:fe00:2659%eth0/onie-installer-VENDOR\_MACHINE

http://fe80::4638:39ff:fe00:2659%eth0/onie-installer-powerpc

http://fe80::4638:39ff:fe00:2659%eth0/onie-installer

http://fe80::230:48ff:fe9f:1547%eth0/onie-installer-powerpc-VENDOR\_MACHINE-r0

http://fe80::230:48ff:fe9f:1547%eth0/onie-installer-powerpc-VENDOR\_MACHINE

http://fe80::230:48ff:fe9f:1547%eth0/onie-installer-VENDOR\_MACHINE

http://fe80::230:48ff:fe9f:1547%eth0/onie-installer-powerpc

http://fe80::230:48ff:fe9f:1547%eth0/onie-installer

### TFTP waterfall

The firmware shall include a classic PXE-like TFTP waterfall method for locating a NOS installer image. Given a TFTP server address, the firmware will attempt to download the installer using a sequence of TFTP paths with decreasing levels of specificity.

An example of this method is as follows:

55-66-aa-bb-cc-dd/onie-installer-<arch>-<vendor>\_<machine>

C0A801B2/onie-installer-<arch>-<vendor>\_<machine>

C0A801B/onie-installer-<arch>-<vendor>\_<machine>

C0A801/onie-installer-<arch>-<vendor>\_<machine>

C0A80/onie-installer-<arch>-<vendor>\_<machine>

C0A8/onie-installer-<arch>-<vendor>\_<machine>

C0A/onie-installer-<arch>-<vendor>\_<machine>

C0/onie-installer-<arch>-<vendor>\_<machine>

C/onie-installer-<arch>-<vendor>\_<machine>

onie-installer-<arch>-<vendor>\_<machine>-<machine\_revision>

onie-installer-<arch>-<vendor>\_<machine>

onie-installer-<vendor>\_<machine>

onie-installer-<arch>

onie-installer

## NOS Uninstallation

The firmware is required to allow a user to completely remove the current NOS installed leaving only the firmware intact. The firmware will wipe out all unused portions of NOR flash and the attached mass storage device (like an SD card or USB NAND flash). The only thing untouched is the firmware itself. This is akin to ‘reset to factory defaults’.

## Update ONIE

The firmware is required to provide a facility to self-update via the same method used in NOS image discovery and installation except for a firmware image rather than a NOS image.

The firmware is required to discover an ONIE image through the following methods (in order):

1. Statically configured (passed from boot loader)
2. Local file systems (USB for example)
3. Exact URLs from DHCPv4
4. Inexact URLs based on DHCP responses
5. IPv6 neighbors
6. TFTP waterfall

### Default File Name Search Order

ONIE searches for default file name for the updated image in a specific order. All update methods use the same default file names and search order, which are described in this section.

The default ONIE image file names are searched for in the following order:

1. onie-updater-<arch>-<vendor>\_<machine>-r<machine\_revision>
2. onie-updater-<arch>-<vendor>\_<machine>
3. onie-updater-<vendor>\_<machine>
4. onie-updater-<arch>
5. onie-updater

### Statically configured (passed from boot loader)

The firmware shall provide this static method as an engineering function to be used during the porting of ONIE to a new platform. To use this method, a statically configured updater URL (install\_url) shall be set by the user on the kernel command line argument prior to booting ONIE. Additional kernel command line arguments can be added by setting the onie\_debugargs environment variable.

### Local file systems (USB for example)

The firmware shall provide a method to identify a locally attached storage device to obtain a firmware updater. This method is intended for the case where the new firmware image is available on a USB memory stick (if supported by the device) plugged into the front panel. The supported file systems the firmware will support shall be vfat (common on commercially available USB sticks) and ext2.

The general algorithm for locating the installer on local storage proceeds as follows:

foreach $partition in /proc/partitions {

if able to mount $partition then {

if default file name exists {

Add partition to found\_list

}

}

}

foreach $partition in found\_list {

Run updater from $partition

}

### Exact URLs from DHCPv4

The firmware shall provide a method to use a URL from a DHCPv4 response. Please refer to the section above for details.

### Inexact URLs based on DHCP responses

The firmware can find an updater using partial DHCP information by using a default sequence of URL paths and default file names in conjunction with partial DHCP information available to find an updater image. Please refer to the section above for details.

### IPv6 neighbors

The firmware shall also query its IPv6 link-local neighbors via HTTP for an updater image. Please refer to the section above for details.

### TFTP waterfall

The firmware shall include a classic PXE-like TFTP waterfall method for locating an updated firmware image. Given a TFTP server address, the firmware will attempt to download the updater using a sequence of TFTP paths with decreasing levels of specificity.

An example of this method is as follows:

55-66-aa-bb-cc-dd/onie-updater-<arch>-<vendor>\_<machine>

C0A801B2/onie-updater-<arch>-<vendor>\_<machine>

C0A801B/onie-updater-<arch>-<vendor>\_<machine>

C0A801/onie-updater-<arch>-<vendor>\_<machine>

C0A80/onie-updater-<arch>-<vendor>\_<machine>

C0A8/onie-updater-<arch>-<vendor>\_<machine>

C0A/onie-updater-<arch>-<vendor>\_<machine>

C0/onie-updater-<arch>-<vendor>\_<machine>

C/onie-updater-<arch>-<vendor>\_<machine>

onie-updater-<arch>-<vendor>\_<machine>-<machine\_revision>

onie-updater-<arch>-<vendor>\_<machine>

onie-updater-<vendor>\_<machine>

onie-updater-<arch>

onie-updater

## Rescue Mode

The firmware is required to provide a rescue mode as a failsafe, to perform diagnostics and to reload a new NOS. The rescue mode is the same as the discovery and installation phase, but the discovery mechanism is disabled. The firmware shall not try to locate and install a NOS image, but rather allow troubleshooting of the current system.

In this mode of operation, the firmware is accessible via the serial console or via telnet. A user can use the available BusyBox toolset to attempt to fix the problem or use wget to retrieve additional resources.

## Execution Environment

After the firmware locates and downloads an installer, the next step is to execute the installer.

Prior to execution, the firmware prepares an execution environment:

1. chmod +x on the downloaded installer
2. Export a number of environment variables (defined below) which are usable by the installer
3. Executes the installer

|  |  |
| --- | --- |
| Variable Name | Meaning |
| onie\_exec\_url | Currently executing URL |
| onie\_platform | CPU architecture, vendor and machine name |
| onie\_vendor\_id | 32-bit IANA Private Enterprise Number |
| onie\_serial\_num | Device serial number |
| onie\_eth\_addr | MAC address for Ethernet management port |
| onie\_version | ONIE build version number |

Table - Installer Core Environment Variables

In addition to the environment variables, any and all DHCP response options are exported, in the style of BusyBox’s udhcpc. Those variables are as follows:

|  |  |
| --- | --- |
| Variable Name | Meaning |
| onie\_disco\_dns | DNS Server |
| onie\_disco\_domain | Domain name from DNS |
| onie\_disco\_hostname | Switch hostname |
| onie\_disco\_interface | Ethernet management interface (i.e. eth0) |
| onie\_disco\_ip | Ethernet management IP address |
| onie\_disco\_router | Gateway |
| onie\_disco\_serverid | DHCP server IP |
| onie\_disco\_siaddr | TFTP server IP |
| onie\_disco\_subnet | IP netmask |
| onie\_disco\_vivso | VIVSO option data |

Table - Installer DHCP Environment Variables

# ONIE Testing

## Test Environment

In order to test an ONIE device, the following is required:

* ONIE device
* Vendor provided serial console cable (for device interaction and recording of session)
* CAT5/CAT6 RJ45 cable (for image discovery and delivery)
* PC with serial terminal and RJ45 NIC

Recommended environment - Linux

* Latest Linux distribution (e.g. Debian) with IPv6 enabled
* screen(1) or minicom(1)
  + 115200 baud 8N1, no flow control
  + Logging enabled
* ISC DHCP Server
  + See Appendix A – dhcpd.conf example file or <https://github.com/onie/onie/blob/master/contrib/isc-dhcpd/dhcpd.conf>
* Web Server
  + Apache httpd
  + nginx
  + lighttpd
* TFTP server
  + atftpd
* USB memory stick (if supported by the device)
  + 2GB is sufficient

Recommended environment - Windows

* Windows 8.1 Update
* PuTTY or Tera Term
  + 115200 baud 8N1, no flow control
  + Logging enabled
* dhcpsrv (<http://www.dhcpserver.de/dhcpsrv.htm>)
  + Also includes web server and tftp server
* Web Server
  + IIS
  + Apache httpd
* TFTP server
  + WinAgents TFTP server
* USB memory stick (if supported by the device)
  + 2GB is sufficient

## Dead on Arrival Testing

Prior to the start of the testing the ONIE device, the ONIE Certification lab will be performing the following functionality testing

1. Power on the switch, perform any vendor diagnostic test, if applicable.
2. Verify the hardware configuration such as CPU, memory, flash storage, USB, Network ports, labeling and asset tracking
3. Perform warm reboot 20 x AC power cycles
4. Perform cold boot 20 x AC power cycles

**PASS Criteria: Switch boots from warm and cold boot. Tests 0 and 1.**

## Manual Testing

### Preliminary

Before putting a device under test, it is best to know the available environment variables and options as they will be used in a variety of ways (naming schemes for install and update images, host options, etc…). Below is a print out of using the printenv command from UBoot.

LOADER=> printenv

autoload=no

baudrate=115200

bootargs=root=/dev/ram rw console=ttyS0,115200 quiet

bootcmd=run check\_boot\_reason; run nos\_bootcmd; run onie\_bootcmd

bootdelay=10

check\_boot\_reason=if test -n $onie\_boot\_reason; then setenv onie\_bootargs boot\_reason=$onie\_boot\_reason; run onie\_bootcmd; fi;

consoledev=ttyS0

dhcp\_user-class=powerpc-as4600\_54t\_uboot

dhcp\_vendor-class-identifier=powerpc-as4600\_54t

ethact=eth0

ethaddr=70:72:CF:AA:34:FA

ethprime=eth0

gatewayip=192.168.1.10

hostname=es4654bf\_zz-unknown

ipaddr=192.168.1.10

loadaddr=0x2000000

loads\_echo=1

netmask=255.255.255.0

nos\_bootcmd=echo

onie\_args=run onie\_initargs onie\_platformargs

onie\_bootcmd=echo Loading Open Network Install Environment ...; echo Platform: $onie\_platform ; echo Version : $onie\_version ; cp.b $onie\_start $loadaddr ${onie\_sz.b} && run onie\_args && bootm ${loadaddr}#$platform

onie\_initargs=setenv bootargs quiet console=$consoledev,$baudrate

onie\_machine=as4600\_54t

onie\_machine\_rev=0

onie\_platform=powerpc-as4600\_54t

onie\_platformargs=setenv bootargs $bootargs serial\_num=${serial#} eth\_addr=$ethaddr $onie\_bootargs $onie\_debugargs

onie\_rescue=setenv onie\_boot\_reason rescue && boot

onie\_start=0xefB60000

onie\_sz.b=0x00400000

onie\_uninstall=setenv onie\_boot\_reason uninstall && boot

onie\_update=setenv onie\_boot\_reason update && boot

onie\_vendor\_id=259

platform=as4600\_54t

serial#=460054T1406013

serverip=192.168.1.99

stderr=serial

stdin=serial

stdout=serial

ver=U-Boot 2013.01.01-g73423af-dirty (Jan 10 2014 - 21:00:23) - 3.0.1.6

Environment size: 1584/65532 bytes

LOADER=>

Of interest for testing,

|  |  |
| --- | --- |
| Variable | Value |
| MAC Address | 70:72:CF:AA:34:FA |
| arch | powerpc |
| vendor | 259 |
| machine | as4600\_54t |
| machine\_revision | 0 |

Table - ONIE Variables from Device

### NOS image discovery and Installation

#### Statically configured (passed from boot loader)

Prior to booting into ONIE, the environment variable install\_url needs to be set. To ensure ONIE will perform the installation regardless if there is a NOS installed, the variable onie\_boot\_reason needs to be set to install .

LOADER=> setenv onie\_boot\_reason install

LOADER=> setenv onie\_debugargs install\_url=<URL>

LOADER=> boot

**PASS Criteria: ONIE installs the specified image. Test 2.**

#### Local file systems (USB for example)

Prior to booting ONIE, a USB memory stick with an ONIE image conforming to the naming scheme above. Boot device. This test is only valid for those devices that contain a USB port.

**PASS Criteria: ONIE installs image from USB device using all options of the naming scheme. Tests 3 – 7.**

#### Exact URLs from DHCPv4

Prior to booting ONIE, ensure the ONIE image server has the DHCP server configured to parse out VIVSO (defined above) and other DHCP options. When using default-url, please ensure the appropriate service (ftp, http, or tftp) is enabled.

**PASS Criteria: ONIE installs image using Exact URLs from DHCPv4 (all 4 targets). Tests 8 – 11.**

#### Inexact URLs based on DHCP responses

Prior to booting ONIE, ensure the ONIE image server has the DHCP server configured with four options (configured one at a time). Please refer to Inexact URLs based on DHCP responses for the four options. All options except for the TFTP bootfile, will locate the image by conforming to the naming scheme defined above.

**PASS Criteria: ONIE installs image using Inexact URLs from 4 DHCPv4 options (all 16 tests). Tests 12 – 27.**

#### IPv6 neighbors

Prior to booting ONIE, ensure the ONIE image server has IPv6 configured and running a web server with the ONIE images conforming to the naming scheme above.

**PASS Criteria: ONIE installs image from IPv6 neighbor device using all options of the naming scheme. Tests 28 – 32.**

#### TFTP waterfall

Prior to booting ONIE, ensure the ONIE image server has the TFTP service enabled and configured.

**PASS Criteria: ONIE installs image from TFTP waterfall using all options of the naming scheme. Tests 33 – 37.**

### NOS Uninstallation

To perform the NOS uninstallation will depend on where in the boot process the device is in.

If the device is powered off:

* Boot device
* Break out to UBoot prompt

LOADER=> run onie\_uninstall

Otherwise

# fw\_setenv onie\_boot\_reason uninstall

# reboot

**PASS Criteria: ONIE boots up and performs the uninstallation phase erasing all blocks of the previous image. Tests 74 – 76.**

### Update ONIE

#### Statically configured (passed from boot loader)

Prior to booting into ONIE, the environment variable install\_url needs to be set. To ensure ONIE will perform the upgrade regardless if there is a NOS installed, the variable onie\_boot\_reason needs to be set to update .

LOADER=> setenv onie\_boot\_reason update

LOADER=> setenv onie\_debugargs install\_url=<URL>

LOADER=> boot

**PASS Criteria: ONIE installs the specified image. Test 38.**

#### Local file systems (USB for example)

Prior to booting ONIE, a USB memory stick with an ONIE image conforming to the naming scheme above. Boot device. This test is only valid for those devices that contain a USB port.

**PASS Criteria: ONIE updates image from USB device using all options of the naming scheme. Tests 39 – 43.**

#### Exact URLs from DHCPv4

Prior to booting ONIE, ensure the ONIE image server has the DHCP server configured to parse out VIVSO (defined above) and other DHCP options. When using default-url, please ensure the appropriate service (ftp, http, or tftp) is enabled.

**PASS Criteria: ONIE updates image using Exact URLs from DHCPv4 (all 4 targets). Tests 44 – 47.**

#### Inexact URLs based on DHCP responses

Prior to booting ONIE, ensure the ONIE image server has the DHCP server configured with four options (configured one at a time). Please refer to Inexact URLs based on DHCP responses for the four options. All options except for the TFTP bootfile, will locate the image by conforming to the naming scheme defined above.

**PASS Criteria: ONIE updates image using Inexact URLs from 4 DHCPv4 options (all 16 tests). Tests 48 – 63.**

#### IPv6 neighbors

Prior to booting ONIE, ensure the ONIE image server has IPv6 configured and running a web server with the ONIE images conforming to the naming scheme above.

**PASS Criteria: ONIE updates image from IPv6 neighbor device using all options of the naming scheme. Tests 64 – 68.**

#### TFTP waterfall

Prior to booting ONIE, ensure the ONIE image server has the TFTP service enabled and configured.

**PASS Criteria: ONIE updates image from TFTP waterfall using all options of the naming scheme. Tests 69 – 73.**

### Rescue Mode

To enter rescue mode will depend on where in the boot process the device is in.

If the device is powered off:

* Boot device
* Break out to UBoot prompt

LOADER=> run onie\_rescue

Otherwise:

# fw\_setenv onie\_boot\_reason rescue

# reboot

**PASS Criteria: ONIE boots up without the discover mechanism running. Tests 77 – 79. Verify with boot screen saying:**

**discover: Rescue mode detected. Installer disabled.**

**Or via** ps w**.**

# Appendix A – dhcpd.conf example file

# Sample configuration demonstrating many ONIE install options

ddns-update-style none;

option domain-name "ocp-labs.local";

option domain-name-servers 192.168.1.1;

default-lease-time 600;

max-lease-time 7200;

# Create an option namespace called ONIE for VIVSO (option 125)

option space onie code width 1 length width 1;

# Define the code names and data types within the ONIE namespace

option onie.installer\_url code 1 = text;

option onie.updater\_url code 2 = text;

option onie.machine code 3 = text;

option onie.arch code 4 = text;

option onie.machine\_rev code 5 = text;

# Package the ONIE namespace into option 125

option space vivso code width 4 length width 1;

option vivso.onie code 42623 = encapsulate onie;

option vivso.iana code 0 = string;

option op125 code 125 = encapsulate vivso;

# Optionally add syslog server for logging

# option log-servers 192.168.1.3;

log-facility local7;

# Logging constructs to assist with debugging

log(error, concat("vendor-class: ", substring(option vendor-class-identifier, 0, 11)));

log(error, concat("platform : ", substring(option vendor-class-identifier, 12, 999)));

# Parses vendor-class-identifier and adjusts the default-url

class "onie-vendor-X-class" {

match if substring(option vendor-class-identifier, 0, 27) = "onie\_vendor:powerpc-VendorX";

option default-url = "http://onie-server/VendorX-onie-installer";

}

# VIVSO example

class "onie-vendor-classes" {

# Limit the matching to a request we know originated from ONIE

match if substring(option vendor-class-identifier, 0, 11) = "onie\_vendor";

# Required to use VIVSO

option vivso.iana 01:01:01;

# generic CPU architecture matching

if option onie.arch = "powerpc" {

option onie.installer\_url = "http://onie-server/generic-powerpc-onie-installer";

}

# matching on CPU architecture and machine type

if option onie.arch = "powerpc" and option onie.machine = "XYZ1234" {

option onie.installer\_url = "http://onie-server/powerpc-xyz1234-onie-installer";

}

# The contents of an option can also be used to create the response text

if exists onie.arch and exists onie.machine and exists onie.machine\_rev {

option onie.installer\_url = concat("http://onie-server/image-installer-",

option onie.arch, "-", option onie.machine,

"-r", option onie.machine\_rev);

}

# When operating in ONIE 'update' mode ONIE will check the

# onie.updater\_url response option

if option onie.arch = "powerpc" and option onie.machine = "XYZ1234" {

option onie.updater\_url = "http://onie-server/onie-updater-VENDOR\_XYZ1234-powerpc.bin";

}

}

# Uses the default-url option for ONIE

subnet 192.168.1.0 netmask 255.255.255.0 {

range 192.168.1.150 192.168.1.240;

authoritative;

option routers 192.168.1.1;

option broadcast-address 192.168.1.255;

option default-url = "http://192.168.1.2/custom-onie-installer";

# Below is the same but uses DNS resolution

# option default-url = "http://onie-server/custom-onie-installer";

}

# Typical tftp waterfall example

# ONIE will also try to use HTTP on the next-server and dhcpd server

subnet 192.168.1.0 netmask 255.255.255.0 {

range 192.168.1.150 192.168.1.240;

authoritative;

option routers 192.168.1.1;

option broadcast-address 192.168.1.255;

next-server 192.168.1.1;

}